UMON CERN Program Library Z020

Author(s) : F. Carminati Library: KERNLIB, VAX/VMS only Submitter : Submitted: 01.03.1989 Language : VAX Fortran Revised: Usage Monitor for VAX/VMS

UMCOM is an usage monitor package for VAX/VMS systems. Usage log requests are performed either via

Fortran calls or via DCL commands. Structure:

Complete PROGRAM and SUBROUTINE subprograms User Entry Names: UMCOM, UMLOG Usage:

   CALL UMCOM(CMD,MONITOR,TEXT)

CMD (CHARACTER) The ^rst two letters of CMD are interpreted as a command to UMON. See the

Long Write-up for possible commands.

MONITOR (CHARACTER) Name of the monitor to be affected by the command. If this name is longer

than 8 characters, only the ^rst 8 will be taken into account.

TEXT (CHARACTER) A character string containing information about the command given. If this

string is longer than 80 characters, only the ^rst 80 will be taken into account.

   CALL UMLOG(MONITOR,TEXT)

MONITOR (CHARACTER) Name of the monitor to be affected by the command. If this name is longer

than 8 characters, only the ^rst 8 will be taken into account.

TEXT (CHARACTER) A character string containing the text to be logged. If this string is longer than

80 characters, only the ^rst 80 will be taken into account.

See also the Long Write-up. ffl

1 Z020 Ű 1