INCBYT CERN Program Library M423 Author(s) : J. Zoll, P. Rastl Library: KERNLIB Submitter : Submitted: 28.01.1971 Language : Fortran or Assembler Revised: 16.09.1991 Increment a Byte of a Packed Vector

INCBYT allows incrementing a speci^ed byte of a packed byte vector (cf. PACBYT (M422)).

Structure:

FUNCTION subprogram

User Entry Names: INCBYT Usage:

LOST = INCBYT(INC,MX,JX,MPACK)

The 3-word vector MPACK speci^es the packing parameters (much like for PACBYT (M422), but NBITS = 0 is not allowed):

MPACK(1) ≡ NBITS, number of bits per byte.
MPACK(2) ≡ INWORD, number of bytes per word.
MPACK(3) ≡ MAXCAP, the maximum capacity of any byte, ≤ 2**NBITS−1.
INCBYT adds the increment INC into the JX’th byte of the packed byte-vector MX and returns any byte

over~ow, i.e. the part of INC which cannot be added into the byte, because it now contains MPACK(3). •

1 M423 Ű 1